20210415

* The yaw angle return to zero logic need to be verified √
* The load cell, potentiometer and IMU need to be calibrated, spring stiffness also need to be calibrated
* IMU need to check if it is 6 axis or 9 axis
* System parameter and motor + driver actuation unit parameter calibration
* High-level controller end condition