20210420

* Check if every information from sensor and corresponding calculation is correct before implement controller
* High-level logic and thresholds are waited to be checked and determined

20210421

* Record expected initial value of every sensor